**QMK Firmware flashing tutorial**

1. Download QMK TOOLBOX from [Releases · qmk/qmk\_toolbox (github.com)](https://github.com/qmk/qmk_toolbox/releases) and install it.



1. Run QMK Toolbox as administrator.



3.In QMK Toolbox click on open button and Select QMK Firmware file as shown below: 

4.After select the file, keep the MCU (AVR only) in ATmega32U4 ,Press and hold CTRL+ESC, then connect the wire then click on Flash button in QMK Toolbox. Then it displays like below figure



5. Click on «Exit DFU»  
6. Reconnect the keyboard  
  
P.S.  
  
If you see this error on your screen, select this item.

